# Kernel config based on: arch/arm/configs/peregrine_defconfig

pkgname="linux-motorola-peregrine"
pkgver=3.4.113
pkgrel=1
pkgdesc="Moto G 4G (2013) kernel fork"
arch="armhf"
_carch="arm"
_flavor="motorola-peregrine"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
depends="libsparse"
makedepends="coreutils perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev xz dtbtool"
HOSTCC="${CC:-gcc}"
HOSTCC="${HOSTCC#${CROSS_COMPILE}}"

# Source
_repository="android_kernel_motorola_msm8226"
_commit="75e7c47f8084a89b3b3019641aea9f01166bfbcb"
_config="config-${_flavor}.${arch}"
source="
	$pkgname-$_commit.tar.gz::https://github.com/LineageOS/${_repository}/archive/${_commit}.tar.gz
	$_config
	compiler-gcc6.h
	00_fix_return_address.patch
	02_gpu-msm-fix-gcc5-compile.patch
	03_mdss_fb_refresh_rate.patch
	06_fix_mdss_fb_rgb_mode.patch
"
builddir="$srcdir/${_repository}-${_commit}"

prepare() {
	default_prepare

	# gcc6 support
	cp -v "$srcdir/compiler-gcc6.h" "$builddir/include/linux/"

	# Remove -Werror from all makefiles
	find . -type f -name Makefile -print0 | \
		xargs -0 sed -i 's/-Werror-/-W/g'
	find . -type f -name Makefile -print0 | \
		xargs -0 sed -i 's/-Werror//g'

	# Prepare kernel config ('yes ""' for kernels lacking olddefconfig)
	cp "$srcdir"/$_config "$builddir"/.config
	yes "" | make ARCH="$_carch" HOSTCC="$HOSTCC" oldconfig
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"

	# Generate master DTB
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm/boot/dt.img" "arch/arm/boot/"
}

package() {
	# kernel.release
	install -D "$builddir/include/config/kernel.release" \
		"$pkgdir/usr/share/kernel/$_flavor/kernel.release"

	# zImage (find the right one)
	cd "$builddir/arch/$_carch/boot"
	_target="$pkgdir/boot/vmlinuz-$_flavor"
	for _zimg in zImage-dtb Image.gz-dtb *zImage Image; do
		[ -e "$_zimg" ] || continue
		msg "zImage found: $_zimg"
		install -Dm644 "$_zimg" "$_target"
		break
	done
	if ! [ -e "$_target" ]; then
		error "Could not find zImage in $PWD!"
		return 1
	fi

	# We need the dtb file
	install -Dm644 "$builddir/arch/arm/boot/dt.img" \
		"$pkgdir/boot/dt.img"
}

sha512sums="8e651741fce8b6263647ae3f91bbd8ac6d36178ba1bd7c7dc31829e52596efc151ea344c43413a322b28ba96a8cc81def4b70e502940d50a92f66a1a18b263a9  linux-motorola-peregrine-75e7c47f8084a89b3b3019641aea9f01166bfbcb.tar.gz
4a31482b0182565c09b1c5a42c3c6058caa7bce76beac007c1bea8b0afa97fa42cb2bc2fade3043201d672cb3fcdd3dc4d138784c196e2868470fb877801a7ed  config-motorola-peregrine.armhf
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h
ea1d3b5a234fa565e3c1a792de48f4fc4e6023d281d303c8e319c7ef28edc5739ab0e4dea0139a41f0a5c7d03e27921ccaa214fd0ac5c72245a094ce60128864  00_fix_return_address.patch
7be03a9e78b7ac330a54b1f00509caa0621a95c0c55901878ad757f9dd69cc05ba2c8b5ea987063ae1224f92c4d090d515fa5d369e7755181a4871b0d0f82881  02_gpu-msm-fix-gcc5-compile.patch
a8c955bf718f155011e980f3d0948be98e1fee5649f418299a4851780543019daf7afa406aa7b0829375645107e4e6fbf241026b0cabe2b2ac895a47df83d2d8  03_mdss_fb_refresh_rate.patch
384ae0bf2f5d7e15b0b60655693fd600b52c0f5bfcaa4ba7336d0ebeb224e84b99b597f77d26a1249e14a4e7bbc1629be00556b393bb9dd2266cb4bd67c3cfea  06_fix_mdss_fb_rgb_mode.patch"
