From ab272bfc9aef6d50c44e1c1bdfdb8a325aebaefc Mon Sep 17 00:00:00 2001
From: Khem Raj <raj.khem@gmail.com>
Date: Fri, 7 Jul 2017 15:12:39 -0700
Subject: [PATCH] chromium: musl: Use correct member name __si_fields from
 LinuxSigInfo

Signed-off-by: Khem Raj <raj.khem@gmail.com>
---
 chromium/sandbox/linux/seccomp-bpf/trap.cc | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/3rdparty/chromium/sandbox/linux/seccomp-bpf/trap.cc b/src/3rdparty/chromium/sandbox/linux/seccomp-bpf/trap.cc
index 003708d2c8..0fef3148f9 100644
--- a/src/3rdparty/chromium/sandbox/linux/seccomp-bpf/trap.cc
+++ b/src/3rdparty/chromium/sandbox/linux/seccomp-bpf/trap.cc
@@ -168,7 +168,7 @@ void Trap::SigSys(int nr, LinuxSigInfo* info, ucontext_t* ctx) {
   // most versions of glibc don't include this information in siginfo_t. So,
   // we need to explicitly copy it into a arch_sigsys structure.
   struct arch_sigsys sigsys;
-  memcpy(&sigsys, &info->_sifields, sizeof(sigsys));
+  memcpy(&sigsys, &info->__si_fields, sizeof(sigsys));
 
 #if defined(__mips__)
   // When indirect syscall (syscall(__NR_foo, ...)) is made on Mips, the
