# Kernel config based on: arch/arm64/configs/athene_defconfig

pkgname="linux-motorola-athene"
pkgver=3.10.108
pkgrel=0
pkgdesc="Motorola Moto G4 kernel fork"
arch="aarch64"
_carch="arm64"
_flavor="motorola-athene"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev dtbtool xz"
HOSTCC="${CC:-gcc}"
HOSTCC="${HOSTCC#${CROSS_COMPILE}}"

# Source
_repository="android_kernel_motorola_msm8952"
_commit="4f6c8d2e1507595b5ef404d076128874176f1219"
_config="config-${_flavor}.${arch}"
source="
	$pkgname-$_commit.tar.gz::https://github.com/fengjiongmax/${_repository}/archive/${_commit}.tar.gz
	$_config
	compiler-gcc6.h
	01_fix_gcc6_errors.patch
"
builddir="$srcdir/${_repository}-${_commit}"

prepare() {
	default_prepare

	# gcc6 support
	cp -v "$srcdir/compiler-gcc6.h" "$builddir/include/linux/"

	# Remove -Werror from all makefiles
	local i
	local makefiles="$(find . -type f -name Makefile)
		$(find . -type f -name Kbuild)"
	for i in $makefiles; do
		sed -i 's/-Werror-/-W/g' "$i"
		sed -i 's/-Werror//g' "$i"
	done

	# Prepare kernel config ('yes ""' for kernels lacking olddefconfig)
	cp "$srcdir"/$_config "$builddir"/.config
	yes "" | make ARCH="$_carch" HOSTCC="$HOSTCC" oldconfig
}

menuconfig() {
	cd "$builddir"
	make ARCH="$_carch" menuconfig
	cp .config "$startdir"/$_config
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"

	# Generate master DTB (deviceinfo_bootimg_qcdt)
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm64/boot/dt.img" "arch/arm64/boot/"
}

package() {
	# kernel.release
	install -D "$builddir/include/config/kernel.release" \
		"$pkgdir/usr/share/kernel/$_flavor/kernel.release"

	# zImage (find the right one)
	cd "$builddir/arch/$_carch/boot"
	_target="$pkgdir/boot/vmlinuz-$_flavor"
	for _zimg in zImage-dtb Image.gz-dtb *zImage Image; do
		[ -e "$_zimg" ] || continue
		msg "zImage found: $_zimg"
		install -Dm644 "$_zimg" "$_target"
		break
	done
	if ! [ -e "$_target" ]; then
		error "Could not find zImage in $PWD!"
		return 1
	fi

	# Master DTB (deviceinfo_bootimg_qcdt)
	install -Dm644 "$builddir/arch/arm64/boot/dt.img" \
		"$pkgdir/boot/dt.img"
}

sha512sums="74d13e6787337454dc09c643efcf95cd46a2f02deecbe687c7a451f53bc2a5978aca394cf76f828cced88a6cffb310deb430c2c8c989471b368733f1aad728c2  linux-motorola-athene-4f6c8d2e1507595b5ef404d076128874176f1219.tar.gz
806b21e3057815e1fe97ebf5950ff9ea800d69c4bd7ef5127a89927c9f6042bd7c51524e20319cfdfd651694dac3999aec453af9143ec2f4e36a5634b5d2946a  config-motorola-athene.aarch64
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h
972e98523d6ef06342e69a09e979bdd86904cf7f9a843b519b37791e531b680182564a2ab537c94629c3589f4e775b2c39de04c64e210a0f8b6f10745c3596f1  01_fix_gcc6_errors.patch"
