# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Wileyfox Swift"
deviceinfo_manufacturer="Wileyfox"
deviceinfo_codename="wileyfox-crackling"
deviceinfo_year="2015"
deviceinfo_dtb_mainline="qcom/msm8916-longcheer-l8150"
deviceinfo_dtb_mainline_modem="qcom/msm8916-longcheer-l8150-modem"
deviceinfo_append_dtb_mainline="true"
deviceinfo_append_dtb_mainline_modem="true"
deviceinfo_modules_initfs_downstream=""
deviceinfo_modules_initfs_mainline="panel-booyi-otm1287 msm rmi_i2c qcom-spmi-vadc dumb-adc-battery"
deviceinfo_modules_initfs_mainline_modem="panel-booyi-otm1287 msm rmi_i2c qcom-spmi-vadc dumb-adc-battery"
deviceinfo_arch="aarch64"

# Device related
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="720"
deviceinfo_screen_height="1280"
deviceinfo_dev_touchscreen="/dev/input/event3"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_kernel_cmdline_mainline="earlycon=msm_serial_dm,0x78b0000 console=ttyMSM0,115200,n8 PMOS_NO_OUTPUT_REDIRECT"
deviceinfo_kernel_cmdline_mainline_modem="earlycon=msm_serial_dm,0x78b0000 console=ttyMSM0,115200,n8 PMOS_NO_OUTPUT_REDIRECT"
deviceinfo_kernel_cmdline_downstream="console=ttyHSL0,115200,n8 androidboot.console=ttyHSL0 androidboot.hardware=qcom msm_rtb.filter=0x237 ehci-hcd.park=3 androidboot.bootdevice=7824900.sdhci lpm_levels.sleep_disabled=1 loop.max_part=7 buildvariant=userdebug"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt_downstream="true"
deviceinfo_flash_offset_base="0x80000000"
deviceinfo_flash_offset_kernel="0x00080000"
deviceinfo_flash_offset_ramdisk="0x02000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x01e00000"
deviceinfo_flash_pagesize="2048"
deviceinfo_flash_sparse="true"
