# Contributor: Asriel Dreemurr <asriel.danctnix@gmail.com>
# Contributor: Danct12 <danct12@disroot.org>
# Contributor: pinoaffe
# Maintainer: Asriel Dreemurr <asriel.danctnix@gmail.com>
# Maintainer: Danct12 <danct12@disroot.org>

# Reference: <https://postmarketos.org/devicepkg>
pkgname="device-xiaomi-santoni"
pkgdesc="Xiaomi Redmi 4X"
pkgver=0.5
pkgrel=5
url="https://postmarketos.org"
license="MIT"
arch="aarch64"
options="!check !archcheck"
depends="postmarketos-base linux-xiaomi-santoni mkbootimg mesa-dri-swrast msm-fb-refresher"
makedepends="devicepkg-dev"
subpackages="$pkgname-nonfree-firmware:nonfree_firmware
		$pkgname-nonfree-userland:nonfree_userland
		$pkgname-hybris:hybris
		$pkgname-hybris-x11:hybris_x11"
source="
	hybris/10-santoni-android-x11.conf
	hybris/70-santoni-android.rules
	hybris/fstab.android
	misc/100-charging.rules
	misc/charging.sh
	misc/discharging.sh
	ucm/90-device-xiaomi-santoni-audio.rules
	ucm/HiFi
	ucm/msm8920-sku7-snd-card.conf
	deviceinfo
	directfbrc
	fb.modes"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname

	install -Dm644 "$srcdir"/fb.modes "$pkgdir"/etc/fb.modes
	install -Dm644 "$srcdir"/directfbrc "$pkgdir"/etc/directfbrc

	install -Dm755 "$srcdir"/charging.sh "$pkgdir"/usr/lib/device-xiaomi-santoni/charging.sh
	install -Dm755 "$srcdir"/discharging.sh "$pkgdir"/usr/lib/device-xiaomi-santoni/discharging.sh
	install -Dm644 "$srcdir"/100-charging.rules \
		"$pkgdir"/etc/udev/rules.d/100-charging.rules

	# Disable v4l udev rules (video4linux), because without the camera
	#         firmware blobs this makes udev helper hang (#1033)
	mkdir -p "$pkgdir"/etc/udev/rules.d
	ln -s /dev/null "$pkgdir"/etc/udev/rules.d/60-persistent-v4l.rules

}

nonfree_firmware() {
	pkgdesc="Wi-Fi, ADSP Firmware (DON'T INSTALL IF USE **LIBHYBRIS**)"
	depends="firmware-xiaomi-santoni wcnss-wlan adsp-audio pulseaudio pulseaudio-alsa alsa-plugins-pulse alsa-utils"
	install="$pkgname-nonfree-firmware.post-install"
	mkdir "$subpkgdir"

	# Install UCM files for santoni
	install -Dm644 "$srcdir"/HiFi \
		"$subpkgdir"/usr/share/alsa/ucm2/msm8920-sku7-snd-card/HiFi
	install -Dm644 "$srcdir"/msm8920-sku7-snd-card.conf \
		"$subpkgdir"/usr/share/alsa/ucm2/msm8920-sku7-snd-card/msm8920-sku7-snd-card.conf
	install -Dm644 "$srcdir"/90-device-xiaomi-santoni-audio.rules \
		"$subpkgdir"/etc/udev/rules.d/90-device-xiaomi-santoni-audio.rules
}

nonfree_userland() {
	pkgdesc="Pulls libhybris (Android) hardware adaptation, see the device's wiki page for post-install."
	depends="$pkgname-hybris"
	mkdir "$subpkgdir"
}

hybris() {
	pkgdesc="libhybris (Android) hardware adaptation"
	depends="hybris-base pulseaudio-modules-droid-7.1-caf alsa-plugins-pulse alsa-utils"
	install="$pkgname-hybris.post-install"

	mkdir "$subpkgdir"

	# Android mounts (needed for loading firmware and configs from android container)
	# Appended to fstab in post-install script
	install -Dm644 "$srcdir"/fstab.android "$subpkgdir"/etc/fstab.android

	# Android udev rules, depend on android users and groups presence
	install -Dm644 "$srcdir"/70-santoni-android.rules \
		"$subpkgdir"/etc/udev/rules.d/70-santoni-android.rules
}

hybris_x11() {
	pkgdesc="X11 modules for libhybris adaptation"
	depends="hybris-base-x11-caf"
	install_if="$pkgname-hybris xorg-server"

	# X11 Hybris configuration
	install -Dm644 "$srcdir"/10-santoni-android-x11.conf \
		"$subpkgdir"/etc/X11/xorg.conf.d/10-santoni-android-x11.conf
}
sha512sums="dc68956408da82ac9775f23814fb6e1498e65a4c760ceda369a60a202cfc92ad27761d6da27f1802307042affc8a1925c576816a8acbf394dd6a15f32e3ea3c0  10-santoni-android-x11.conf
7c0cda58ddc36e8a6120ce969c1e7afc445817e20b38a4c33e986d3d584bcf0fbb4d82eeda4dab5abdf3429845621a4ffa155512f40e885be615042faf1de171  70-santoni-android.rules
8419c1c5d20bc7c7e4d8d72ec2848655526f99cabf9037ae1f7152f5df31363b70b724769225a88c1d614bea6ebe4ee24190702ea947229a843cc2884eac7175  fstab.android
7b1b138372cb173be38e820a1c386c3d30930d6753303478ae08c1362de3099d81c26eb2b833c5a0b340a82d821bd53309058ecb9b62e00c7ff323b632af2346  100-charging.rules
c4853babd5cd6371297e5e5d64364c064d540cd4beaba06d79b1001fe5c78fe3ee8bc5f6f4ba3e383743a09263028abc55f41bad45240b1c505e27ed087725c9  charging.sh
6012be4184af6c4f12f9b20a6f2d377ebd72b9b334df4fbb921ed9d8da865633631f77d19b02748ebee70442e2f3ffcb6af511ee5deaa40635bc53730c301076  discharging.sh
dc4bf7871307e659f220aebc3c9f7d74b861f46e1f3df1be37d724af984e46d91e553dbd36c2bd4482aa17dbe4d76d28dabe214952638f00830907466b110146  90-device-xiaomi-santoni-audio.rules
3452fe367e7b199d610fb3d8e9113b35e04071afc7585080edb6fe584ecc29591d8f3ab53ed4583c1ccea5882aa51050d6e56a5db7ef88f6c9af648ba1ef88af  HiFi
7c702cf159699cea761ce7cb1ca21b79c59ceb3cdf1e410b537c4aa3a5aaa3be171b4c5555a713ac7a0e0f6dc389680cd5368a7783d14025fdc14d5f27fb922b  msm8920-sku7-snd-card.conf
4aea469f7980900c2ffee2a3e77bf280cf722a5580425c545d25236cd8d1add1a6613ae9f73222d35554d1ccb8a2446220e0af244970894ad581bdcf79fb32df  deviceinfo
3db3ec596e159be926ea2b5b2496c18e9bc7be24a64a232a56c89a0c9ee710aa2efb2b6fa9fc08efa34759e8242e6c629d08a4ce688ec8aa125830717c191515  directfbrc
b634d13cac1f10535a31c142c7391986ab402ae9910d8093989920f4c2dbd63722ee8595f11962bffd9d314e2835a1ead955a91355856f044911ddcf1e428427  fb.modes"
