# Kernel config based on: arch/arm64/configs/potter_defconfig

pkgname="linux-motorola-potter"
pkgver=3.18.91
pkgrel=2
pkgdesc="Motorola Moto G5 Plus kernel fork"
arch="aarch64"
_carch="arm64"
_flavor="motorola-potter"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev devicepkg-dev dtbtool xz gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="android_kernel_motorola_msm8953"
_commit="5ec24e0225d19f2746088c88fbbc48978da5f3d5"
_config="config-$_flavor.$arch"
source="
	$pkgname-$_commit.tar.gz::https://github.com/boulzordev/android_kernel_motorola_msm8953/archive/$_commit.tar.gz
	$_config
	01_prima_gcc6.patch
	02_fix_msm_dba.patch
	03_fix_rndis_ipa_trace_header_not_found.patch
	04_fix_stmvl53l0_headers.patch
	05_fix_u_f_header.patch
	06_fix_usb_gadget_function.patch
	compiler-gcc6.h
"
builddir="$srcdir/$_repository-$_commit"

prepare() {
	default_prepare
	. downstreamkernel_prepare
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"
	# Generate master DTB
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm64/boot/dt.img" "arch/arm64/boot/"
}

package() {
	downstreamkernel_package "$builddir" "$pkgdir" "$_carch" "$_flavor"

	# Master DTB
	install -Dm644 "$builddir/arch/arm64/boot/dt.img" \
		"$pkgdir/boot/dt.img"
}

sha512sums="e735870e981e727afd0fb97c3ae5e544a724cbf6024c6ad710fca7e50bb19a613b42a40d1f9ec18f449d8b9c85cba9d5713b472b4204c74b5ba893f2b7e61749  linux-motorola-potter-5ec24e0225d19f2746088c88fbbc48978da5f3d5.tar.gz
98429151eebf0d071d0db487d8d8a9acdcebafb3b3634cb207a74400a1136ea0f824f8c327cb8cf853688fe31a14c1af6f50050f3ec5d907f81d5576d88aed8c  config-motorola-potter.aarch64
184875cf13a180d1c4bbe27d8ad24a8d6bd2e36ec35f9c4326809f1c8938ecebf3844c36ef71f4a0af9077e2506a82b2b4383ffd020dd1918aba1689d77b0c01  01_prima_gcc6.patch
7e765cb696fa8c3dfbc305b05cbf1fad85fb9572613d5391e945341dae5974a745f4906c795dc841e5562b19ab77d5257f9741e514af2c2573aa4bb8b262ce51  02_fix_msm_dba.patch
9c549714f03c7a7666e8aa7508a48cfdccab7cf3e97fb59c4df8fa97f75492365926f82c4a677c50780d68d4905504dcccbdd6de6344bd8d4b88b2331933ed46  03_fix_rndis_ipa_trace_header_not_found.patch
1a128e1483459144726458175314c58528e6b1f1a85e5f4230fa0461b0c3dd650037567f672c220a95618f9df023a82a35f010e8e8b784e349806516c1daaf7e  04_fix_stmvl53l0_headers.patch
b408f157cc025d410b38f5aee9be977e670e1ac3f195f6c3a6681446fa0c3887067d62a4f729cfcd058fab42fca355b0265764dc2d21515f6e023ed025f55d41  05_fix_u_f_header.patch
1f23466d1a864f2d2c67ae4250b0c166ecb7755779bbdad6732808a001cc2826cc1d013c2281d2ca1d5abd7d60d13783f0b9f11bb8359971f2b30b911e627220  06_fix_usb_gadget_function.patch
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h"
