# Reference: <https://postmarketos.org/devicepkg>
# Contributor: Ingo Feinerer <feinerer@logic.at>
pkgname="device-htc-protou"
pkgdesc="HTC Desire X"
pkgver=0.1
pkgrel=3
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="postmarketos-base linux-htc-protou mkbootimg mesa-dri-swrast msm-fb-refresher"
makedepends="devicepkg-dev"
subpackages="$pkgname-nonfree-firmware:nonfree_firmware"
source="deviceinfo initfs-hook.sh pointercal"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname

	install -Dm644 "$srcdir"/pointercal \
		"$pkgdir"/etc/pointercal

	# Disable v4l (video4linux), because without the camera firmware
	# blobs this makes udev hang with the kernel this device uses (#1033)
	ln -s /dev/null "$pkgdir"/etc/udev/rules.d/60-persistent-v4l.rules
}

nonfree_firmware() {
	pkgdesc="Wifi firmware"
	depends="firmware-aosp-broadcom-wlan"
	mkdir "$subpkgdir"
}

sha512sums="62ad386ec0f4cbf80ada7ea7adc042797e23c80d4c7615ed64322198335dc1f2b963a89a5a7d8d76e5c07248a0ed745bbf5df2fddc918ec7827870c0856ff2b3  deviceinfo
b49562b112ac966896d152ba30548f5b863cc94359fb02a8b75ec43a2c1229a852a218d50201628c0cbee3b88b68136163716e78dcc4ec71401ff9dc8340e016  initfs-hook.sh
e76d0a2e1a9b611e811f6c0c90201f019ef435132ea4e7119e6179ffc99ba72c5fb6c3bdd1041ff06186d75a163bf3443d0c073c7fe1b55c10b58af53ada163a  pointercal"
