# Contributor: TAKIZAWA Fumiya <takizawa.fumiya34@gmail.com>
# Reference: <https://postmarketos.org/devicepkg>
pkgname="device-sharp-shl22"
pkgdesc="SHARP SHL22"
pkgver=0.1
pkgrel=1
url="https://postmarketos.org"
license="MIT"
arch="armv7"
options="!check !archcheck"
depends="postmarketos-base linux-sharp-shl22 mesa-dri-swrast mkbootimg msm-fb-refresher"
makedepends="devicepkg-dev"
source="
	deviceinfo
	initfs-hook.sh
"

build() {
	devicepkg_build $startdir $pkgname
}

package() {
	devicepkg_package $startdir $pkgname

	# Disable v4l (video4linux), because without the camera firmware
	# blobs this makes dev hang with the kernel this device uses (#1033)
	mkdir -p "$pkgdir"/etc/udev/rules.d
	ln -s /dev/null "$pkgdir"/etc/udev/rules.d/60-persistent-v4l.rules
}


sha512sums="e8ce0a34dec989bfab4d44e55d1fb2611d2460da58b19dd8e5a7c05ef431dbfc16ef751abc3047b74799ea3af6541773c2b9f199985de1bea1789e9e254060d8  deviceinfo
c983fc8281167bed1de5eec3651d82ed0dea612a4267acc8edf34ac8b1f857a57d5d63c555a373749eef3119cbfc9f4d25a080c0291d5af847642b5f60fcb211  initfs-hook.sh"
