pkgname=firmware-chuwi-hi10plus
pkgver=0.1
pkgrel=2
_commit="2ab861d875105d0b88402d596e3d197dd47135df"
pkgdesc="Firmware for Chuwi Hi10 Plus"
url="https://github.com/onitake/gsl-firmware"
arch="x86_64"
license="proprietary"
source="$pkgname-$_commit.tar.gz::https://github.com/Danct12/gsl-firmware/archive/$_commit.tar.gz
	20-touchscreen-firmware.files"
options="!strip !check !archcheck !spdx"
builddir="$srcdir/gsl-firmware-$_commit"

package() {
	install -Dm644 firmware/chuwi/hi10_plus/firmware.fw \
		"$pkgdir"/lib/firmware/silead/gsl1680-chuwi-hi10plus.fw
	install -Dm644 "$srcdir"/20-touchscreen-firmware.files \
		"$pkgdir"/etc/postmarketos-mkinitfs/files/20-touchscreen-firmware.files
}

sha512sums="5d2f447403941475542aac6110086117ddf031ad96cf1081cc7c63db465c609e2983c34f269fce86598198ab68826f8c8768232aedb8eaaa4b9a61037c61e610  firmware-chuwi-hi10plus-2ab861d875105d0b88402d596e3d197dd47135df.tar.gz
85eda4c0a90f4d9aaf34dff36b08534e27962acd0214873a6b73039a663dd5bfd7de084833b07f2a56314466e2466ad68ce7b6ecbfe496c0578020847bc9b6e6  20-touchscreen-firmware.files"
