From fbc4ce7a84e59215914a8981afe918002b191493 Mon Sep 17 00:00:00 2001
From: Arthur Demchenkov <spinal.by@gmail.com>
Date: Fri, 21 Dec 2018 09:23:57 +0300
Subject: [PATCH] ARM: dts: n900: increase charge current limit to 950mA

That was default in Maemo Fremantle
---
 arch/arm/boot/dts/omap3-n900.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/omap3-n900.dts b/arch/arm/boot/dts/omap3-n900.dts
index de7a31ae72207..7028a7cb2849e 100644
--- a/arch/arm/boot/dts/omap3-n900.dts
+++ b/arch/arm/boot/dts/omap3-n900.dts
@@ -700,7 +700,7 @@
 		ti,current-limit = <100>;
 		ti,weak-battery-voltage = <3400>;
 		ti,battery-regulation-voltage = <4200>;
-		ti,charge-current = <650>;
+		ti,charge-current = <950>;
 		ti,termination-current = <100>;
 		ti,resistor-sense = <68>;
 
