# Maintainer: Martijn Braam <martijn@brixit.nl>
pkgname=crust
pkgver=0.3_git20210418
pkgrel=0
_commit="23d6d7b4fbb5375845d96f622e82435064343098"
pkgdesc="SCP firmware for sunxi SoCs"
arch="aarch64"
url="https://github.com/crust-firmware/crust"
license="BSD-1-Clause AND BSD-3-Clause AND GPL-2.0-only and MIT"
makedepends="gcc-or1k-elf binutils-or1k-elf dtc bison flex"
source="https://github.com/crust-firmware/crust/archive/$_commit/crust-$_commit.tar.gz"
options="!check !archcheck !tracedeps pmb:cross-native" # No tests
builddir="$srcdir/$pkgname-$_commit"

build() {
	make CROSS_COMPILE=or1k-elf- pinephone_defconfig
	make CROSS_COMPILE=or1k-elf- build/scp/scp.bin
}

package() {
	install -D -m644 build/scp/scp.bin "$pkgdir"/usr/share/crust/pinephone/scp.bin
}
sha512sums="
15058a888f10b9434eea76951acd44010bc6628d911c9cbbf043d5b8c26a4d226d24cc6fda3698b093d7ccb055a6c047d146410ca4cd2d44040c622b6aad2568  crust-23d6d7b4fbb5375845d96f622e82435064343098.tar.gz
"
