# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Motorola Moto X4"
deviceinfo_manufacturer="Motorola"
deviceinfo_codename="motorola-payton"
deviceinfo_year="2017"
deviceinfo_dtb=""
deviceinfo_modules_initfs=""
deviceinfo_arch="aarch64"

# Device related
deviceinfo_chassis="handset"
deviceinfo_keyboard="false"
deviceinfo_external_storage="true"
deviceinfo_screen_width="1080"
deviceinfo_screen_height="1920"

# Bootloader related
deviceinfo_flash_method="fastboot"
deviceinfo_kernel_cmdline="console=ttyMSM0,115200,n8 androidboot.console=ttyMSM0 earlycon=msm_serial_dm,0xc170000 androidboot.hardware=qcom user_debug=31 msm_rtb.filter=0x37 ehci-hcd.park=3 lpm_levels.sleep_disabled=1 sched_enable_hmp=1 sched_enable_power_aware=1 service_locator.enable=1 swiotlb=1 androidboot.configfs=true androidboot.usbcontroller=a800000.dwc3 androidboot.hab.csv=2 androidboot.hab.product=payton androidboot.hab.cid=50 androidboot.fastboot=1 buildvariant=eng"
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="false"
deviceinfo_bootimg_dtb_second="false"
deviceinfo_flash_offset_base="0x00000000"
deviceinfo_flash_offset_kernel="0x00008000"
deviceinfo_flash_offset_ramdisk="0x01000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x00000100"
deviceinfo_flash_pagesize="4096"
deviceinfo_flash_sparse="true"

# USB related
deviceinfo_usb_rndis_function="rndis_bam.rndis"
