From 18ffb110c41738fb8661cd0c98749b89c26daa3d Mon Sep 17 00:00:00 2001
From: Martijn Braam <martijn@brixit.nl>
Date: Mon, 15 Feb 2021 13:10:37 -0800
Subject: [PATCH] pinephone: fix pogopin i2c

---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 6 +-----
 1 file changed, 1 insertion(+), 5 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index 1a096576d258..4abda4fac41f 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -645,11 +645,7 @@ &pio {
 	vcc-pb-supply = <&reg_dcdc1>;
 	vcc-pc-supply = <&reg_dcdc1>;
 	vcc-pd-supply = <&reg_dcdc1>;
-	/* pinctrl would enable this even if no camera is powered,
-	 * which is wrong/not necessary
-	 *
-	 * vcc-pe-supply = <&reg_aldo1>; (also used by pogo pins i2c)
-	 */
+	vcc-pe-supply = <&reg_aldo1>; /* (also used by pogo pins i2c) */
 	vcc-pf-supply = <&reg_dcdc1>;
 	vcc-pg-supply = <&reg_dldo4>;
 	vcc-ph-supply = <&reg_dcdc1>;
-- 
2.31.1

