# Kernel config based on: arch/arm/configs/elementalx_defconfig

pkgname=linux-asus-duma
pkgver=3.4.113
pkgrel=5
pkgdesc="ASUS MeMO Pad FHD 10 (ME302KL) kernel fork"
arch="armhf"
_carch="arm"
_flavor="asus-duma"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps pmb:cross-native"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev devicepkg-dev xz gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="ElementalX-Kernel-for-ME302KL"
_commit="b6a8f08e43a26771947556abfc697971eb67f06b"
_config="config-$_flavor.$arch"
source="
	$pkgname-$_commit.tar.gz::https://github.com/yatto/$_repository/archive/$_commit.tar.gz
	$_config
	00_fix_return_address.patch
	02_gpu-msm-fix-gcc5-compile.patch
"
builddir="$srcdir/$_repository-$_commit"

prepare() {
	default_prepare
	. downstreamkernel_prepare
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"
}

package() {
	downstreamkernel_package "$builddir" "$pkgdir" "$_carch" "$_flavor"
}

sha512sums="f47c0dfb34f9387ce9b7518fee6cae2fd91161cf1db0f0355bbc87fb201798d8c87f78779d3df4022a9bceeac8d9f0b111f7e63f25394e3f8cfbcd57a9da48c6  linux-asus-duma-b6a8f08e43a26771947556abfc697971eb67f06b.tar.gz
6cb6370ef9c54e3b9933a4ba2a3435604315ee27767ca5f3436398a9265d54dcfda73420ca5cdc9c96b0d42547146f4a14f7d17c1d0c446747c8a60d39e6aad0  config-asus-duma.armhf
ea1d3b5a234fa565e3c1a792de48f4fc4e6023d281d303c8e319c7ef28edc5739ab0e4dea0139a41f0a5c7d03e27921ccaa214fd0ac5c72245a094ce60128864  00_fix_return_address.patch
7be03a9e78b7ac330a54b1f00509caa0621a95c0c55901878ad757f9dd69cc05ba2c8b5ea987063ae1224f92c4d090d515fa5d369e7755181a4871b0d0f82881  02_gpu-msm-fix-gcc5-compile.patch"
