From dd52b971005271d615e63f4f946a0ee9331925bc Mon Sep 17 00:00:00 2001
From: dhivael <dhivael.git@eno.space>
Date: Sat, 11 Jan 2020 15:04:04 +0100
Subject: [PATCH 3/5] rockchip: move mmc1 before mmc0 in default boot order

on pinebooks mmc1 is the external card, which should take boot priority
over the internal emmc even if the emmc is bootable.
---
 include/configs/rockchip-common.h | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/include/configs/rockchip-common.h b/include/configs/rockchip-common.h
index 0b9e24d1db4..6610f95b7b9 100644
--- a/include/configs/rockchip-common.h
+++ b/include/configs/rockchip-common.h
@@ -17,8 +17,8 @@
 /* First try to boot from SD (index 0), then eMMC (index 1) */
 #if CONFIG_IS_ENABLED(CMD_MMC)
 	#define BOOT_TARGET_MMC(func) \
-		func(MMC, mmc, 0) \
-		func(MMC, mmc, 1)
+		func(MMC, mmc, 1) \
+		func(MMC, mmc, 0)
 #else
 	#define BOOT_TARGET_MMC(func)
 #endif
-- 
2.25.3

