# Maintainer: Sireesh Kodali <scarface@disroot.org>
pkgname=firmware-motorola-potter
pkgver=1
pkgrel=0
pkgdesc="Firmware for Motorola Moto G5 Plus"
url="https://github.com/scarface-one/firmware-motorola-potter"
arch="aarch64"
depends="linux-firmware-qcom soc-qcom-msm8916-ucm"
license="proprietary"
options="!check !strip !archcheck"
_commit="cce83e64585c036facd4cef39f47bc23d18ba2e9"
builddir="$srcdir/$pkgname-$_commit"

source="$pkgname-$_commit.tar.gz::https://github.com/scarface-one/firmware-motorola-potter/archive/$_commit.tar.gz
	moto-modem-rfs-setup.openrc
	firmware.files
	firmware-motorola-potter.post-install"

package() {
	install -Dm755 $srcdir/moto-modem-rfs-setup.openrc "$pkgdir"/etc/init.d/moto-modem-rfs-setup

	while IFS="" read -r _i || [ -n "$_i" ]; do
		[ ! -d $(dirname $_i) ] && mkdir -p $(dirname $_i)
		echo $_i
		install -Dm644 $_i "$pkgdir/$_i"
	done < "$srcdir/firmware.files"
}
sha512sums="5a35ff1b567b672585f761eddbc772163f52b312c1e94410eff4b1d333852857a2f87769a45f47f7bcff373bdd5b062c3d16110e0211d85f83a7b4c6c78f6d3c  firmware-motorola-potter-cce83e64585c036facd4cef39f47bc23d18ba2e9.tar.gz
d4fd0f3406c9f004e9cae7bc500c5713aab75f102f8e3ea1af820865f01eb03def01cd9ed3e8a184c7dfc22ab419628fad17957a3782885d96eb36e94461e842  moto-modem-rfs-setup.openrc
dc7b179abb099ab61bc72e8941be38d3e94bd1a43b37617b34e1a63835bb8399ee79a87d556996dfbed032e40554ca48a2ff9e9817d80ed1415db3f369266b38  firmware.files
784ac120a2231cfbee153fb8b2634af4ab5091eaa8fe207e66b47641d7531591ee3849e610bb66c7177822c86556f78d51c17ba8e4f3da2f946c4b8c5eaaf310  firmware-motorola-potter.post-install"
