From 1a24e50b7e3538b4ca9dd1a1fe310b1effaf0aaf Mon Sep 17 00:00:00 2001
From: Sergey Larin <cerg2010cerg2010@mail.ru>
Date: Sat, 9 Feb 2019 18:30:12 +0300
Subject: [PATCH] ARM: dts: tegra20-glide: add intrrupt binding for charger

Add missing interrupt for max17043 charger

Signed-off-by: Sergey Larin <cerg2010cerg2010@mail.ru>
---
 arch/arm/boot/dts/tegra20-glide.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/boot/dts/tegra20-glide.dts b/arch/arm/boot/dts/tegra20-glide.dts
index 76493614f6df..cb219d1b1198 100644
--- a/arch/arm/boot/dts/tegra20-glide.dts
+++ b/arch/arm/boot/dts/tegra20-glide.dts
@@ -819,6 +819,8 @@
 		max17043@36 {
 			compatible = "maxim,max17040";
 			reg = <0x36>;
+			interrupt-parent = <&gpio>;
+			interrupts = <TEGRA_GPIO(I, 5) IRQ_TYPE_LEVEL_HIGH>;
 		};
 	};
 
-- 
2.22.0

