# Reference: <https://postmarketos.org/deviceinfo>
# Please use double quotes only. You can source this file in shell scripts.

deviceinfo_format_version="0"
deviceinfo_name="Fairphone 2"
deviceinfo_manufacturer="Fairphone"
deviceinfo_date=""
deviceinfo_keyboard="false"
deviceinfo_nonfree="????"
deviceinfo_dtb=""
deviceinfo_modules=""
deviceinfo_modules_initfs=""
deviceinfo_external_storage="true"
deviceinfo_flash_method="fastboot"
deviceinfo_flash_sparse="true"
deviceinfo_arch="armhf"

# Splash screen
deviceinfo_screen_width="1080"
deviceinfo_screen_height="1920"

# Fastboot related
deviceinfo_generate_bootimg="true"
deviceinfo_bootimg_qcdt="true"

deviceinfo_kernel_cmdline="console=ttyHSL0,115200,n8 PMOS_NO_OUTPUT_REDIRECT"
deviceinfo_flash_offset_kernel="0x00000000"
deviceinfo_flash_offset_ramdisk="0x02000000"
deviceinfo_flash_offset_second="0x00f00000"
deviceinfo_flash_offset_tags="0x01E00000"
deviceinfo_flash_pagesize="2048"

# Weston red screen workaround (see issue #54)
deviceinfo_weston_pixman_type="2"
