# Kernel config based on: arch/arm64/configs/ze550kl_defconfig

pkgname="linux-asus-z00t"
pkgver=3.10.108
pkgrel=2
pkgdesc="Zenfone 2 Laser/Selfie (1080p) kernel fork"
arch="aarch64"
_carch="arm64"
_flavor="asus-z00t"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev devicepkg-dev dtbtool gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="android_kernel_asus_msm8916"
_commit="5fd66aa9219bf9aaa504aa3cb2dae7a3de5238f7"
_config="config-$_flavor.$arch"
source="
	$pkgname-$_commit.tar.gz::https://github.com/LineageOS/$_repository/archive/$_commit.tar.gz
	$_config
	compiler-gcc6.h
	01_fix_gcc6_errors.patch
	02_mdss_fb_refresh_rate.patch
	05_dtb-fix.patch
"
builddir="$srcdir/$_repository-$_commit"

prepare() {
	default_prepare
	. downstreamkernel_prepare
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"

	# Generate master DTB (deviceinfo_bootimg_qcdt)
	dtbTool -s 2048 -p "scripts/dtc/" -o "arch/arm64/boot/dt.img" "arch/arm/boot/"
}

package() {
	downstreamkernel_package "$builddir" "$pkgdir" "$_carch" "$_flavor"

	# Master DTB (deviceinfo_bootimg_qcdt)
	install -Dm644 "$builddir/arch/arm64/boot/dt.img" \
		"$pkgdir/boot/dt.img"
}

sha512sums="2a43545d07b4b477749ac4eaf793e0e7cf105699264d4bd97df20904a3039f421330825dc8c7f9f741387dc3dd9c48b716de6c797048a1f9f358fee97f68fa85  linux-asus-z00t-5fd66aa9219bf9aaa504aa3cb2dae7a3de5238f7.tar.gz
395ec02b12bb376fd558267308b908af9da4111dd18e29639f6c972d8ed2a0cd0a127479adaebe9c618962ea7cddf6d1f63b29b03cd8f5c095c0f9453960f799  config-asus-z00t.aarch64
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h
972e98523d6ef06342e69a09e979bdd86904cf7f9a843b519b37791e531b680182564a2ab537c94629c3589f4e775b2c39de04c64e210a0f8b6f10745c3596f1  01_fix_gcc6_errors.patch
a8c955bf718f155011e980f3d0948be98e1fee5649f418299a4851780543019daf7afa406aa7b0829375645107e4e6fbf241026b0cabe2b2ac895a47df83d2d8  02_mdss_fb_refresh_rate.patch
0e5ebee2f1b0005fcae4f313219c0b6481b3d044c7167e0fb18b72db0eae49aef7b281cd29e0fa1e653fc5585064c990085ca68f920348c3d9d9ea9524d1baa6  05_dtb-fix.patch"
