# Kernel config based on: arch/arm64/configs/lineageos_ether_defconfig

pkgname="linux-nextbit-robin"
pkgver=3.10.108
pkgrel=2
pkgdesc="Nextbit Robin kernel fork"
arch="aarch64"
_carch="arm64"
_flavor="nextbit-robin"
url="https://kernel.org"
license="GPL2"
options="!strip !check !tracedeps"
makedepends="perl sed installkernel bash gmp-dev bc linux-headers elfutils-dev devicepkg-dev gcc6"

# Compiler: this kernel was only tested with GCC6. Feel free to make a merge
# request if you find out that it is booting working with newer GCCs as
# well. See <https://postmarketos.org/vendorkernel> for instructions.
if [ "${CC:0:5}" != "gcc6-" ]; then
	CC="gcc6-$CC"
	HOSTCC="gcc6-gcc"
	CROSS_COMPILE="gcc6-$CROSS_COMPILE"
fi

# Source
_repository="android_kernel_nextbit_msm8992"
_commit="8b8773362248bdba3224a1d92e76c5b9004519d6"
_config="config-$_flavor.$arch"
source="
	$pkgname-$_commit.tar.gz::https://github.com/LineageOS/$_repository/archive/$_commit.tar.gz
	$_config
	compiler-gcc6.h
	01_psci_err.patch
"
builddir="$srcdir/$_repository-$_commit"

prepare() {
	default_prepare
	. downstreamkernel_prepare
}

build() {
	unset LDFLAGS
	make ARCH="$_carch" CC="${CC:-gcc}" \
		KBUILD_BUILD_VERSION="$((pkgrel + 1 ))-postmarketOS"
}

package() {
	downstreamkernel_package "$builddir" "$pkgdir" "$_carch" "$_flavor"
}

sha512sums="f2bffe51d021cbe7e5eb3f33486ee3544ca4477e4d21bfb2cffb5743e16dd24a02dbbb93daa45f43ed1825607b730fb39a1b7dace7b24f99a844dca577ba52ad  linux-nextbit-robin-8b8773362248bdba3224a1d92e76c5b9004519d6.tar.gz
2b1bfe206071852b5866cd932f290650e57866386dbf80f992d9229d287fa5910724ad9486280e0f8c0885adae77ac5cf9803fdc5d5594b524a87ceddd947d7e  config-nextbit-robin.aarch64
d80980e9474c82ba0ef1a6903b434d8bd1b092c40367ba543e72d2c119301c8b2d05265740e4104ca1ac5d15f6c4aa49e8776cb44264a9a28dc551e0d1850dcc  compiler-gcc6.h
8740861d5e125a5f9faa144e6fe6d7e6413250664547f217bf8a02e1bea77f9809582c952cdd3618fcbf150979faab57540ecc3370d6734cc82bbd62afdf15b1  01_psci_err.patch"
