From eef79bbcc6afc2cb4441be760c8e2c06594589df Mon Sep 17 00:00:00 2001
From: Martijn Braam <martijn@brixit.nl>
Date: Tue, 20 Oct 2020 17:58:00 +0200
Subject: [PATCH] dts: pinephone: remove bt firmware suffix

---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 1 -
 1 file changed, 1 deletion(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index 346113382e7d..d3d4f1a53c8d 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -876,7 +876,6 @@ bluetooth {
 		device-wake-gpios = <&pio 7 6 GPIO_ACTIVE_LOW>; /* PH6 */
 		enable-gpios = <&r_pio 0 4 GPIO_ACTIVE_HIGH>; /* PL4 */
 		host-wake-gpios = <&r_pio 0 5 GPIO_ACTIVE_HIGH>; /* PL5 */
-		firmware-postfix = "pinephone";
 	};
 };
 
-- 
2.31.1

